# Server Commands

SkyChart can work as a server. It accepts the following commands from a TCP/IP connection:

## Connection

You can use any socket library or object to connect to Skychart from your software, or use the commands telnet or netcat from a script.
To send a command, write to the socket the command, any parameter separated by a blank space, and finally a CR-LF termination.
For examples with various languages, see https://github.com/pchev/skychart/tree/master/skychart/sample_client

The standard port is 3292, this can be changed by the user in the configuration menu. The program can also choose to listen to another random port if the configured port is busy.

Skychart maintains a file with information about the port and it's status.
In Linux and Mac: [User settings]/tmp/tcpport
In Windows: Registry key HKCU\Software\Astro_PC\Ciel\Status\TcpPort

The file (or key) do not exist if Skychart was never run.
It contains 0 if the program is not running, or the server is disabled in the configuration menu.
It contains the listen port if the program is ready to accept a connection.

## Main Commands

Command | Parameters | Comment or GUI Equivalent
--- | --- | ---
NEWCHART | chart_name | File → New Chart
CLOSECHART | chart_name | File → Close Chart
SELECTCHART | chart_name | Window → chart_name
LISTCHART |  | Window
SEARCH | object_name | Search tool (Main Bar)
GETMSGBOX |  | Returns the status bar content
GETCOORBOX |  | Returns the coordinates shown in the status bar
GETINFOBOX |  | Setup → Display → Labels - Display the chart information in the menu bar
FIND | object_class object_name | Same as search, but lets you specify the class of object you want: 0=nebula, 1=na, 2=star, 3=star, 4=variable, 5=double, 6=comet, 7=asteroid, 8=planet, 9=constellation, 10=line catalog
SAVE | saved_file_name | Save the current chart to the specified file
LOAD | saved_file_name | Load the chart from the file
LOADDEFAULT | option_file_name | Use this command to load an extract of the configuration file that temporarily replace some option from skychart.ini.
SETCAT | path shortname active min max | Add or change a Catgen catalog. The fields are the same as in the catalog setup.
SHUTDOWN |  | Close the program
RESET |  | Reload the default chart and options (same as signal HUP)
PLANETINFO | page_number | Open the Solar system information window at the given page
GETSELECTEDOBJECT |  | Return information about the last selected object
LOADMPCORB | file_name | Load the specified file with asteroid element in MPCORB format. Detail result is available in file [user_data]/database/LoadAsteroidFile.log
? |  | No GUI equivalent, list of available commands

## Chart Commands

Command | Parameters | Comment or GUI Equivalent
--- | --- | ---
ZOOM+ |  | View → Zoom in
ZOOM- |  | View → Zoom out
MOVEEAST |  | Keyboard Left arrow
MOVEWEST |  | Keyboard Right arrow
MOVENORTH |  | Keyboard Up arrow
MOVESOUTH |  | Keyboard Down arrow
MOVENORTHEAST |  | Numpad 7 (Ver num off)
MOVENORTHWEST |  | Numpad 9 (Ver num off)
MOVESOUTHEAST |  | Numpad 1 (Ver num off)
MOVESOUTHWEST |  | Numpad 3 (Ver num off)
FLIPX |  | Chart > Tranformation > Mirror Horizontally
FLIPY |  | Chart > Tranformation > Mirror Vertically
SETCURSOR | pixX pixY |
CENTRECURSOR |  | Right-clic → Center
ZOOM+MOVE |  | Right-clic → Zoom + Move
ZOOM-MOVE |  | Right-clic → Zoom - Move
ROT+ |  | Chart → Tranformation → Rotate Right
ROT- |  | Chart → Tranformation → Rotate Left
SETEQGRID | ON/OFF | Chart → Lines, Grid → Add Equatorial Grid
SETGRID | ON/OFF | Chart → Lines, Grid → Show Coordinate Grid
SETSTARMODE | 0/1/2 | Setup → Display → Display → Star Display
SETNEBMODE | 0/1 | Setup > Display → Display → Deep Sky Objects Display
SETAUTOSKY | ON/OFF | Setup → Display → Sky Colour
UNDO |  | Edit → Undo
REDO |  | Edit → Redo
SETPROJ | ALTAZ/EQUAT/GALACTIC/ECLIPTIC | Chart → Chart Coordinate System
SETFOV | 00d00m00s or 00.00 | Icon (FOV input fields) or icon (Main Bar)
SETRA | RA:00h00m00s or 00.00 | Icon (RA input fields)
SETDEC | DEC:+00d00m00s or 00.00 | Icon (DEC input fields)
SETOBS | LAT:+00d00m00sLON:+000d00m00s ALT:000mOBS:name | Setup → Observatory Beware the longitude must be negative East. In many case you must change the longitude sign.
IDCURSOR |  |
SAVEIMG | PNG/JPEG/BMP filename quality | File → Save Image…
PRINT | PRT/PS/BMP PORTRAIT/LANDSCAPE COLOR/BW filepath | Print or export to Postscript or Bitmap, File → Print and File→ Printer setup
SETNORTH |  | Chart → View Horizon → North
SETSOUTH |  | Chart → View Horizon → South
SETEAST |  | Chart → View Horizon → East
SETWEST |  | Chart → View Horizon → West
SETZENITH |  | Icon (Right Bar)
ALLSKY |  | Icon (Right Bar)
REDRAW |  | Follows a modification command, mandatory to update chart
GETCURSOR |  |
GETEQGRID |  |
GETGRID |  |
GETSTARMODE |  |
GETNEBMODE |  |
GETAUTOSKY |  |
GETPROJ |  |
GETFOV | S/F |
GETRA | S/F | S → 17h07m12s F → 17.11991
GETDEC | S/F |
GETDATE |  |
GETOBS | LAT:+00d00m00sLON:+000d00m00s ALT:000mOBS:name | Beware the longitude is negative East. In many case you must change the longitude sign.
SETDATE | yyyy-mm-ddThh:mm:ss or “yyyy-mm-dd hh:mm:ss” | Setup → Date/Time
SETTZ | Etc/GMT | Setup → Observatory (Country Timezone)
GETTZ |  |
SETGRIDNUM | ON/OFF | Setup → Display → Lines - Show Grid Label
SETCONSTLINE | ON/OFF | Setup → Display → Lines - Show Constellation Figure
SETCONSTBOUNDARY | ON/OFF | Setup → Display → Lines - Show Constellation Boundary
RESIZE | width height | Resize the chart
GETRISESET |  | Get rise/transit/set time for the last selected object
MOVESCOPE | RA Dec [00.00] | Move the telescope cursor to coordinates. RA in decimal hours.
MOVESCOPEH | HourAngle Dec [00.00] | Same as MOVESCOPE but hourangle instead of RA. Hourangle in decimal hours.
IDCENTER |  | Identify object at chart center
IDSCOPE |  | Identify object at telescope cursor position
SHOWPICTURE | ON/OFF | Chart → Show objects → Show pictures
SHOWBGIMAGE | ON/OFF | Show background image
LOADBGIMAGE | fits_filename | Load new background image FITS file, also force reload of updated file if the name is the same.
LOADCIRCLE | file_name | Load a list of finder mark, same as right click - Finder circle - Load from file
SETCIRCLE | num diameter rotation offset | Define a finder circle as in Setup - Display - Finder circle
SETRECTANGLE | num width height rotation offset | Define a finder rectangle as in Setup - Display - Finder rectangle
SHOWCIRCLE | num_list | Set a comma separated list of circle to be activated 1,2,…,10
SHOWRECTANGLE | num_list | Set a comma separated list of rectangle to be activated 1,2,…,10
MARKCENTER | ON/OFF | Show a mark at the chart center, same as Show mark
GETSCOPERADEC |  | Return current telescope coordinates.
TRACKTELESCOPE | ON/OFF | Same as menu Telescope / Track telescope.
CONNECTINDI |  | Connect to configured INDI telescope.
DISCONNECTINDI |  | Disconnect the INDI telescope.
SLEWINDI | RAhr Dec [in decimal] | Slew the INDI telescope to specified coordinates.
ABORTSLEWINDI |  | Abort the current slewing command.
SYNCINDI | RAhr Dec [in decimal] | Sync the INDI telescope at the specified coordinates.
CONNECTTELESCOPE |  | Connect to the default telescope.
DISCONNECTTELESCOPE |  | Disconnect the default telescope.
SLEW | RAhr Dec [in decimal] | Slew the default telescope to specified coordinates.
ABORTSLEW |  | Abort the current slewing command.
SYNC | RAhr Dec [in decimal] | Sync the default telescope at the specified coordinates.
OBSLISTLOAD | list_file_name |
OBSLISTFIRST |  |
OBSLISTLAST |  |
OBSLISTNEXT |  |
OBSLISTPREV |  |
OBSLISTLIMIT | ON/OFF |
OBSLISTAIRMASSLIMIT | [airmass] |
OBSLISTTRANSITLIMIT | [hours] |
OBSLISTTRANSITSIDE | EAST/WEST/BOTH |
GETSCOPERATES |  | Return a list of movement rate supported by the telescope
SCOPEMOVEAXIS | axis(0/1) rate | Start moving the telescope along (axis) using (rate)
SETSCOPEREFRESHRATE | delay [ms] | Refresh the telescope position every (delay) [ms]
PLANISPHEREDATE | ON/OFF | Show or hide the planisphere date scale
PLANISPHERETIME | ON/OFF | Show or hide the planisphere time scale
SETFOVPROJECTION | fov_number HAI/MER/CAR/ARC/TAN/SIN | Set the given projection for the fov_number
SHOWONLYMERIDIAN | ON/OFF | Display only the meridian instead of full grid
SHOWALWAYSMERIDIAN | ON/OFF | Display the meridian line on every projection
CLEANUPMAP |  | Remove any selection and redraw the map
GETCHARTEQSYS |  | Return the current equatorial system for the chart, Date or J2000, B1950, …
GETFRAMES |  | Return the mosaic frames, same as the mosaic tool “Send via server” button

## V2.7 compatibility DDE command

Command | Parameters | Comment or GUI Equivalent
--- | --- | ---
MOVE | obsolete RA: 00h00m00.00s DEC:+00d00m00.0s FOV:+00d00m00s | Icon
DATE | obsolete, same as SETDATE |
OBSL | obsolete, same as SETOBS |
RFSH | obsolete, same as REDRAW |
PDSS |  | Same as the menu Chart-Get DSS Image
SBMP | obsolete, use SAVEIMG |
SGIF | obsolete, use SAVEIMG |
SJPG | obsolete, use SAVEIMG |
IDXY | X:pixelx Y:pixely |
GOXY | X:pixelx Y:pixely |
ZOM+ | obsolete, same as ZOOM+ |
ZOM- | obsolete, same as ZOOM- |
STA+ |  | icon (Main Bar)
STA- |  | icon (Main Bar)
NEB+ |  | icon (Main Bar)
NEB- |  | icon (Main Bar)
GREQ | obsolete, use SETEQGRID |
GRAZ | obsolete, use SETGRID |
GRNM | obsolete, use SETGRIDNUM |
CONL | obsolete, use SETCONSTLINE |
CONB | obsolete, use SETCONSTBOUNDARY |
EQAZ | obsolete, use SETPROJ |

## Information about selected object

The following information are returned when an object is selected on the chart, either by a mouse click or as a result of a search. Each field is separated by the <tab> character.

    > Chart_1 : 23h21m39.85s +61°19'04.8" Nb  NGC 7635 m:11.00 Dim: 15.0 x  8.0 ' class:  Identifier:C11,LBN 548

- > indicate the start of a message.
- Chart_1 : the name of the chart the object was selected.
- 23h21m39.85s RA of the object using current chart equinox.
- +61°19'04.8“ Dec of the object using current chart equinox.
- Nb the type of object
- NGC 7635 the name of the object

Then follow a number of fields whose content depend on the object type and the catalog in use.

If the selection is from a mouse click you can also get this information about the distance from the last selected object:

    > Chart_1 : From: "Sh 2-150" to "NGC 7635 " Separation: +06°48'05.6" PA:119° Offset:  0h49m46.4s -03°53'47"