$BUILT 2016-09-24 14:52:06
$AUTHOR rubix
$ENGLISH Concrete solution

#INTENDED_NUMBER_OF_PLAYERS 1
#SIZE_X 1572
#SIZE_Y 432
#START_X 176
#START_Y 12
#BACKGROUND_RED 0
#BACKGROUND_GREEN 64
#BACKGROUND_BLUE 64

#INITIAL 50
#REQUIRED 42
#SPAWN_INTERVAL 43

#CLIMBER 1
#FLOATER 5
#BUILDER 4
#PLATFORMER 3
#BASHER 2
#MINER 2
#CUBER 8
#EXPLODER2 0

:geoo/construction/Hatch.H: 176 16
:geoo/construction/Hatch.H: 976 64 r

:geoo/construction/Goal2.G: 944 304

:geoo/construction/sawblade.F: 272 288
:geoo/construction/sawblade.F: 368 320
:geoo/construction/sawblade.F: 416 320
:geoo/construction/sawblade.F: 288 288
:geoo/construction/sawblade.F: 304 288
:geoo/construction/sawblade.F: 320 288
:geoo/construction/sawblade.F: 336 304
:geoo/construction/sawblade.F: 352 320
:geoo/construction/sawblade.F: 384 320
:geoo/construction/sawblade.F: 400 320

:geoo/construction/concrete/128: 1024 304
:geoo/construction/concrete/128: 1024 176
:geoo/construction/concrete/032hc: 960 0
:geoo/construction/concrete/128: 1024 48
:geoo/construction/concrete/064h: 1024 -16
:geoo/construction/concrete/032d: 480 336 f
:geoo/construction/concrete/032: 480 368 frr
:geoo/construction/concrete/064h: 512 368
:geoo/construction/concrete/064h: 640 368
:geoo/construction/concrete/064h: 768 368
:geoo/construction/concrete/064h: 192 368
:geoo/construction/concrete/064h: 896 368
:geoo/construction/concrete/064h: 896 112
:geoo/construction/concrete/064h: 1152 176
:geoo/construction/concrete/064h: 1152 320
:geoo/construction/concrete/032hc: 1152 0 frr
:geoo/construction/concrete/016v: 464 336
:geoo/construction/concrete/128: 1440 176
:geoo/construction/concrete/128: 1440 48
:geoo/construction/concrete/128: 1440 304
:geoo/construction/concrete/032hc: 1376 0
:geoo/construction/concrete/064h: 1440 -16
:geoo/construction/concrete/podium_32: 1408 176 rrr
:geoo/construction/concrete/podium_32: 1408 304 rrr
:geoo/construction/concrete/128: 64 240
:geoo/construction/concrete/128: 48 112
:geoo/construction/concrete/128: 48 -16
:geoo/construction/concrete/064h: 192 64
:geoo/construction/concrete/064h: 64 368
:geoo/construction/concrete/032hc: 176 0 frr
:geoo/steel/64x64.S: 1024 176
:geoo/steel/64x64.S: 1088 176
:geoo/steel/64x64.S: 64 176
:geoo/steel/64x64.S: 128 176
:geoo/steel/64x64.S: 1152 176
:geoo/construction/concrete/128: -64 240
:geoo/construction/concrete/064h: -64 368
:geoo/construction/concrete/128: -80 48
:geoo/construction/concrete/064h: -64 176
:geoo/construction/concrete/128: -80 -80
:geoo/steel/64x64.S: 0 176
:geoo/steel/64x64.S: 896 112
:geoo/steel/64x32o.S: 960 144
:geoo/steel/64x64.S: 128 112
:geoo/steel/32x16o.S: 192 112
:geoo/steel/32x16o.S: 224 112
:geoo/construction/concrete/032h: 960 272
:geoo/construction/concrete/032h: 960 256 d
:geoo/construction/concrete/016v: 176 64
:geoo/construction/concrete/016: 176 96
:geoo/steel/16x16o.S: 256 112
