$BUILT 2014-06-06 10:21:50
$AUTHOR Rubix
#INTENDED_NUMBER_OF_PLAYERS 7
$ENGLISH Segmentation Fluctuation (7p)

#SIZE_X 448
#SIZE_Y 1344
#TORUS_X 1
#TORUS_Y 1
#BACKGROUND_RED 0
#BACKGROUND_GREEN 0
#BACKGROUND_BLUE 0

#SECONDS 50
#INITIAL 85
#REQUIRED 24
#SPAWN_INTERVAL 32
#SPAWN_INTERVAL_FAST 4

#CLIMBER 20
#WALKER 60
#JUMPER 60
#NOTHING 0
#EXPLODER2 10
#BUILDER 60
#PLATFORMER 20
#MINER 60
#NOTHING 0
#RUNNER 8
#CUBER 15
#BATTER 25

:geoo/abstract/hatch.H: 368 32
:geoo/abstract/hatch.H: 304 1184
:geoo/abstract/hatch.H: 240 992
:geoo/abstract/hatch.H: 176 800
:geoo/abstract/hatch.H: 112 608
:geoo/abstract/hatch.H: 48 416
:geoo/abstract/hatch.H: 432 224

:geoo/construction/Goal2.G: 96 1168
:geoo/construction/Goal2.G: 32 976
:geoo/construction/Goal2.G: 416 784
:geoo/construction/Goal2.G: 352 592
:geoo/construction/Goal2.G: 288 400
:geoo/construction/Goal2.G: 224 208
:geoo/construction/Goal2.G: 160 16

:geoo/steel/32x16o.S: 176 448 rrr
:geoo/steel/32x16o.S: 48 512
:geoo/steel/32x16o.S: 304 832 rrr
:geoo/steel/32x16o.S: 240 640 rrr
:geoo/steel/32x16o.S: 368 576
:geoo/steel/32x16o.S: 112 704
:geoo/steel/32x16o.S: 432 768
:geoo/steel/32x16o.S: 176 896
:geoo/steel/32x16o.S: 48 960
:geoo/steel/32x16o.S: 304 1280
:geoo/steel/32x16o.S: 240 1088
:geoo/steel/32x16o.S: 112 1152
:geoo/steel/32x16o.S: 432 1216 rrr
:geoo/steel/32x16o.S: 176 0
:geoo/steel/32x16o.S: 48 64 rrr
:geoo/steel/32x16o.S: 304 384
:geoo/steel/32x16o.S: 240 192
:geoo/steel/32x16o.S: 368 128
:geoo/steel/32x16o.S: 112 256 rrr
:geoo/steel/32x16o.S: 432 320
:geoo/construction/stairs_ru_32.S: 112 224
:geoo/construction/stairs_ru_32.S: 176 192
:geoo/construction/stairs_ru_32.S: 240 384
:geoo/construction/stairs_ru_32.S: 176 416
:geoo/construction/stairs_ru_32.S: 240 608
:geoo/construction/stairs_ru_32.S: 304 576
:geoo/construction/stairs_ru_32.S: 48 32
:geoo/construction/stairs_ru_32.S: 112 0
:geoo/construction/stairs_ru_32.S: 304 800
:geoo/construction/stairs_ru_32.S: 368 768
:geoo/construction/stairs_ru_32.S: 432 1184
:geoo/construction/stairs_ru_32.S: 48 1152
:geoo/construction/stairs_ru_32.S: 368 992
:geoo/construction/stairs_ru_32.S: 432 960
:geoo/construction/stairs_ru_32.S: 384 576 frr
:geoo/construction/stairs_ru_32.S: 0 608 frr
:geoo/construction/stairs_ru_32.S: 0 768 frr
:geoo/construction/stairs_ru_32.S: 64 800 frr
:geoo/construction/stairs_ru_32.S: 320 384 frr
:geoo/construction/stairs_ru_32.S: 384 416 frr
:geoo/construction/stairs_ru_32.S: 256 192 frr
:geoo/construction/stairs_ru_32.S: 320 224 frr
:geoo/construction/stairs_ru_32.S: 192 0 frr
:geoo/construction/stairs_ru_32.S: 256 32 frr
:geoo/construction/stairs_ru_32.S: 128 1152 frr
:geoo/construction/stairs_ru_32.S: 192 1184 frr
:geoo/construction/stairs_ru_32.S: 64 960 frr
:geoo/construction/stairs_ru_32.S: 128 992 frr
:geoo/construction/concrete/032h: 48 288
:geoo/construction/concrete/032ha: 432 288
:geoo/construction/concrete/032ha: 48 256
:geoo/construction/concrete/032h: 432 96
:geoo/construction/concrete/032ha: 368 96
:geoo/construction/concrete/032ha: 432 64
:geoo/construction/concrete/032h: 368 1248
:geoo/construction/concrete/032ha: 304 1248
:geoo/construction/concrete/032ha: 368 1216
:geoo/construction/concrete/032h: 304 1056
:geoo/construction/concrete/032ha: 240 1056
:geoo/construction/concrete/032ha: 304 1024
:geoo/construction/concrete/032h: 240 864
:geoo/construction/concrete/032ha: 176 864
:geoo/construction/concrete/032ha: 240 832
:geoo/construction/concrete/032h: 176 672
:geoo/construction/concrete/032ha: 112 672
:geoo/construction/concrete/032ha: 176 640
:geoo/construction/concrete/032h: 112 480
:geoo/construction/concrete/032ha: 48 480
:geoo/construction/concrete/032ha: 112 448
:geoo/steel/32x16o.S: 400 128
:geoo/steel/32x16o.S: 432 128
:geoo/steel/32x16o.S: 32 128 rrr
:geoo/steel/32x16o.S: 16 320
:geoo/steel/32x16o.S: 48 320
:geoo/steel/32x16o.S: 96 320 rrr
:geoo/steel/32x16o.S: 336 1280
:geoo/steel/32x16o.S: 368 1280
:geoo/steel/32x16o.S: 416 1280 rrr
:geoo/steel/32x16o.S: 368 1024 rrr
:geoo/steel/32x16o.S: 272 1088
:geoo/steel/32x16o.S: 304 1088
:geoo/steel/32x16o.S: 352 1088 rrr
:geoo/steel/32x16o.S: 208 896
:geoo/steel/32x16o.S: 240 896
:geoo/steel/32x16o.S: 288 896 rrr
:geoo/steel/32x16o.S: 144 704
:geoo/steel/32x16o.S: 176 704
:geoo/steel/32x16o.S: 224 704 rrr
:geoo/steel/32x16o.S: 80 512
:geoo/steel/32x16o.S: 112 512
:geoo/steel/32x16o.S: 160 512 rrr
:geoo/construction/stairs_ru_32.S: 288 896 frr
:geoo/construction/stairs_ru_32.S: 352 928 frr
:geoo/construction/stairs_ru_32.S: 352 1088 frr
:geoo/construction/stairs_ru_32.S: 416 1120 frr
:geoo/construction/stairs_ru_32.S: 416 1280 frr
:geoo/construction/stairs_ru_32.S: 32 1312 frr
:geoo/construction/stairs_ru_32.S: 32 128 frr
:geoo/construction/stairs_ru_32.S: 96 160 frr
:geoo/construction/stairs_ru_32.S: 96 320 frr
:geoo/construction/stairs_ru_32.S: 160 352 frr
:geoo/construction/stairs_ru_32.S: 160 512 frr
:geoo/construction/stairs_ru_32.S: 224 544 frr
:geoo/construction/stairs_ru_32.S: 224 704 frr
:geoo/construction/stairs_ru_32.S: 288 736 frr
:geoo/steel/32x16o.S: 368 1296 rrr
:geoo/steel/32x16o.S: 368 1328 rrr
:geoo/steel/32x16o.S: 368 16
:geoo/steel/32x16o.S: 400 16
:geoo/steel/16x16o.S: 416 0
:geoo/steel/32x16o.S: 432 144 rrr
:geoo/steel/32x16o.S: 432 176 rrr
:geoo/steel/32x16o.S: 432 208
:geoo/steel/32x16o.S: 16 208
:geoo/steel/16x16o.S: 32 192
:geoo/steel/32x16o.S: 48 368 rrr
:geoo/steel/32x16o.S: 48 400
:geoo/steel/32x16o.S: 80 400
:geoo/steel/16x16o.S: 96 384
:geoo/steel/32x16o.S: 112 528 rrr
:geoo/steel/32x16o.S: 112 560 rrr
:geoo/steel/32x16o.S: 112 592
:geoo/steel/32x16o.S: 144 592
:geoo/steel/16x16o.S: 160 576
:geoo/steel/32x16o.S: 176 720 rrr
:geoo/steel/32x16o.S: 176 752 rrr
:geoo/steel/32x16o.S: 176 784
:geoo/steel/32x16o.S: 208 784
:geoo/steel/16x16o.S: 224 768
:geoo/steel/32x16o.S: 240 912 rrr
:geoo/steel/32x16o.S: 240 944 rrr
:geoo/steel/32x16o.S: 240 976
:geoo/steel/32x16o.S: 272 976
:geoo/steel/16x16o.S: 288 960
:geoo/steel/32x16o.S: 304 1104 rrr
:geoo/steel/32x16o.S: 304 1136 rrr
:geoo/steel/32x16o.S: 304 1168
:geoo/steel/32x16o.S: 336 1168
:geoo/steel/16x16o.S: 352 1152
:geoo/steel/16x16o.S: 112 368
:geoo/steel/16x16o.S: 96 368
:geoo/steel/16x16o.S: 176 560
:geoo/steel/16x16o.S: 160 560
:geoo/steel/16x16o.S: 240 752
:geoo/steel/16x16o.S: 224 752
:geoo/steel/16x16o.S: 304 944
:geoo/steel/16x16o.S: 288 944
:geoo/steel/16x16o.S: 368 1136
:geoo/steel/16x16o.S: 352 1136
:geoo/steel/16x16o.S: 432 1328
:geoo/steel/16x16o.S: 416 1328
:geoo/steel/16x16o.S: 48 176
:geoo/steel/16x16o.S: 32 176
:geoo/steel/32x16o.S: 48 336 rrr
:geoo/construction/concrete/064h: 384 848
:geoo/construction/concrete/064h: 0 1040
:geoo/construction/concrete/064h: 320 656
:geoo/construction/concrete/064h: 256 464
:geoo/construction/concrete/064h: 192 272
:geoo/construction/concrete/064h: 128 80
:geoo/construction/concrete/032h: 304 1296
:geoo/construction/concrete/032h: 304 1328
:geoo/construction/concrete/032ha: 240 1280
:geoo/construction/concrete/032h: 240 1312
:geoo/construction/concrete/032h: 368 144
:geoo/construction/concrete/032h: 368 176
:geoo/construction/concrete/032ha: 304 128
:geoo/construction/concrete/032h: 304 160
:geoo/construction/concrete/032h: 432 336
:geoo/construction/concrete/032h: 432 368
:geoo/construction/concrete/032ha: 368 320
:geoo/construction/concrete/032h: 368 352
:geoo/construction/concrete/032h: 48 528
:geoo/construction/concrete/032h: 48 560
:geoo/construction/concrete/032ha: 432 512
:geoo/construction/concrete/032h: 432 544
:geoo/construction/concrete/032h: 112 720
:geoo/construction/concrete/032h: 112 752
:geoo/construction/concrete/032ha: 48 704
:geoo/construction/concrete/032h: 48 736
:geoo/construction/concrete/032h: 176 912
:geoo/construction/concrete/032h: 176 944
:geoo/construction/concrete/032ha: 112 896
:geoo/construction/concrete/032h: 112 928
:geoo/construction/concrete/032h: 240 1104
:geoo/construction/concrete/032h: 240 1136
:geoo/construction/concrete/032ha: 176 1088
:geoo/construction/concrete/032h: 176 1120
:geoo/abstract/cvblocks/046: 0 1040
:geoo/sandstone/64x32_blank: 128 1264
:geoo/sandstone/64x32_blank: 64 1264
:geoo/sandstone/64x32_blank: 128 1232
:geoo/sandstone/64x32_blank: 64 1232
:simon/tapir/032h: 384 848
:simon/tapir/032h: 0 848
:simon/tapir/032h: 384 880
:simon/tapir/032h: 0 880
:matt/underworld/01: 256 464
:matt/underworld/01: 320 464
:matt/underworld/01: 256 496
:matt/underworld/01: 320 496
:matt/goldmine/crate64: 192 272
:matt/goldmine/crate64: 256 272
:matt/marble/08d: 320 656
:matt/marble/08d: 384 656
:matt/marble/08d: 320 688
:matt/marble/08d: 384 688
:geoo/abstract/cvblocks/035: 240 1312
:geoo/abstract/cvblocks/035: 304 1296
:geoo/abstract/cvblocks/035: 304 1328
:simon/tapir/032h: 240 1104
:simon/tapir/032h: 176 1120
:simon/tapir/032h: 240 1136
:matt/marble/08d: 176 912
:matt/marble/08d: 112 928
:matt/marble/08d: 176 944
:matt/underworld/01: 112 720
:matt/underworld/01: 48 736
:matt/underworld/01: 112 752
:matt/goldmine/crate32: 432 544
:matt/goldmine/crate32: 16 544
:matt/goldmine/crate32: 48 528
:matt/goldmine/crate32: 80 528
:matt/goldmine/crate32: 48 560
:matt/goldmine/crate32: 80 560
:matt/carnival/01: 192 80
:matt/carnival/01: 160 80
:matt/carnival/01: 128 80
:matt/carnival/01: 128 112
:matt/carnival/01: 160 112
:matt/carnival/01: 192 112
:matt/carnival/01: 224 112
:matt/carnival/01: 224 80
:geoo/sandstone/64x32_blank: 368 144
:geoo/sandstone/64x32_blank: 304 160
:geoo/sandstone/64x32_blank: 368 176
:matt/carnival/01: 368 352
:matt/carnival/01: 400 352
:matt/carnival/01: 432 336
:matt/carnival/01: 16 336
:matt/carnival/01: 432 368
:matt/carnival/01: 16 368
:geoo/steel/32x16o.S: 112 1232
:geoo/steel/32x16o.S: 176 80
:geoo/steel/32x16o.S: 240 272
:geoo/steel/32x16o.S: 304 464
:geoo/steel/32x16o.S: 368 656
:geoo/steel/32x16o.S: 432 848
:geoo/steel/32x16o.S: 48 1040
:geoo/construction/concrete/032ha: 128 272
:geoo/construction/concrete/032ha: 320 272 frr
:geoo/construction/concrete/032ha: 64 80
:geoo/construction/concrete/032ha: 0 1232
:geoo/construction/concrete/032ha: 384 1040
:geoo/construction/concrete/032ha: 320 848
:geoo/construction/concrete/032ha: 256 656
:geoo/construction/concrete/032ha: 192 464
:geoo/construction/concrete/032ha: 256 80 frr
:geoo/construction/concrete/032ha: 192 1232 frr
:geoo/construction/concrete/032ha: 128 1040 frr
:geoo/construction/concrete/032ha: 64 848 frr
:geoo/construction/concrete/032ha: 0 656 frr
:geoo/construction/concrete/032ha: 384 464 frr
:geoo/construction/concrete/032ha: 320 304 rr
:geoo/construction/concrete/032ha: 128 304 f
:geoo/construction/concrete/032ha: 384 496 rr
:geoo/construction/concrete/032ha: 0 688 rr
:geoo/construction/concrete/032ha: 64 880 rr
:geoo/construction/concrete/032ha: 128 1072 rr
:geoo/construction/concrete/032ha: 192 1264 rr
:geoo/construction/concrete/032ha: 256 112 rr
:geoo/construction/concrete/032ha: 64 112 f
:geoo/construction/concrete/032ha: 0 1264 f
:geoo/construction/concrete/032ha: 384 1072 f
:geoo/construction/concrete/032ha: 320 880 f
:geoo/construction/concrete/032ha: 256 688 f
:geoo/construction/concrete/032ha: 192 496 f
:geoo/construction/stairs_ru_32.S: 256 1216 frr
:geoo/construction/stairs_ru_32.S: 320 64 frr
:geoo/construction/stairs_ru_32.S: 384 256 frr
:geoo/construction/stairs_ru_32.S: 0 448 frr
:geoo/construction/stairs_ru_32.S: 64 640 frr
:geoo/construction/stairs_ru_32.S: 128 832 frr
:geoo/construction/stairs_ru_32.S: 192 1024 frr
:geoo/steel/16x16o.S: 432 112
:geoo/steel/16x16o.S: 368 1264
:geoo/steel/16x16o.S: 304 1072
:geoo/steel/16x16o.S: 240 880
:geoo/steel/16x16o.S: 176 688
:geoo/steel/16x16o.S: 112 496
:geoo/steel/16x16o.S: 48 304
