$BUILT 2016-05-29 23:04:12
$AUTHOR geoo
$ENGLISH Marching Band

#INTENDED_NUMBER_OF_PLAYERS 1
#SIZE_X 640
#SIZE_Y 400

#INITIAL 50
#REQUIRED 40
#SPAWN_INTERVAL 8

#WALKER 10
#CLIMBER 10
#FLOATER 10
#EXPLODER 10
#PLATFORMER 10
#BATTER 10

:geoo/construction/Hatch.H: 64 208
:geoo/construction/Hatch.H: 528 192 r

:geoo/construction/Goal2.G: 160 32
:geoo/construction/Goal2.G: 416 32

:geoo/construction/spring.T: 304 144

:geoo/construction/concrete/032ha: 192 208
:geoo/construction/concrete/032hb: 96 240
:geoo/construction/concrete/128: 256 272
:geoo/construction/concrete/128: 384 272
:geoo/construction/concrete/128: 128 272
:geoo/construction/concrete/podium_32: 288 176
:geoo/construction/concrete/032ha: 480 240
:geoo/construction/concrete/032hb: 384 208
:geoo/construction/concrete/064h: 256 208
:geoo/construction/concrete/032h: 384 240
:geoo/construction/concrete/032h: 192 240
:geoo/construction/concrete/032b: 448 240
:geoo/construction/concrete/032a: 160 240
:geoo/construction/concrete/032a: 64 240
:geoo/construction/concrete/032b: 544 240
:geoo/construction/concrete/032va: 32 272
:geoo/construction/concrete/032vb: 576 272
:geoo/construction/concrete/064v: 512 272
:geoo/construction/concrete/064v: 64 272
:geoo/construction/concrete/032b: 608 336
:geoo/construction/concrete/032a: 0 336
:geoo/construction/concrete/032v: 32 336
:geoo/construction/concrete/032v: 576 336
:geoo/construction/concrete/032: 0 368
:geoo/construction/concrete/032: 608 368
:geoo/construction/rod_steel/end_rect_du.S: 290 133 rr
:geoo/construction/rod_steel/straight_diagd32.S: 260 96
:geoo/construction/rod_steel/link_du_h.S: 376 84
:geoo/construction/rod_steel/straight_diagu32.S: 342 102
:geoo/construction/rod_steel/end_rect_dd.S: 334 126 fr
:geoo/construction/rod_steel/link_h_dd.S: 244 96
:geoo/construction/rod_steel/straight_diagu32.S: 344 100
:geoo/construction/rod_steel/straight32.S: 392 96
:geoo/construction/rod_steel/straight32.S: 216 96
:geoo/construction/rod_steel/straight32.S: 184 96
:geoo/construction/rod_steel/straight32.S: 152 96
:geoo/construction/rod_steel/straight32.S: 424 96
:geoo/construction/rod_steel/straight32.S: 456 96
:geoo/construction/rod_steel/end_rect.S: 144 96
:geoo/construction/rod_steel/end_rect.S: 488 96 frr
