$BUILT 2014-04-16 21:42:57
$AUTHOR Rubix
#INTENDED_NUMBER_OF_PLAYERS 2
$ENGLISH Containment Problems (2p)

#SIZE_X 832
#SIZE_Y 400
#TORUS_X 0
#TORUS_Y 0
#START_X 96
#START_Y -20
#BACKGROUND_RED 0
#BACKGROUND_GREEN 0
#BACKGROUND_BLUE 0

#SECONDS 45
#INITIAL 80
#REQUIRED 1
#SPAWN_INTERVAL 32
#SPAWN_INTERVAL_FAST 4

#CLIMBER 20
#FLOATER 20
#WALKER 70
#JUMPER 70
#EXPLODER2 10
#BUILDER 80
#PLATFORMER 40
#BASHER 40
#MINER 40
#DIGGER 40
#BATTER 25
#CUBER 5

:geoo/construction/Hatch.H: 672 0 r
:geoo/construction/Hatch.H: 128 0

:geoo/construction/Goal2.G: 144 240
:geoo/construction/Goal2.G: 624 240

:geoo/construction/Laser_hz_64.F: 32 288
:geoo/construction/Laser_hz_64.F: 736 288
:geoo/construction/Laseremit_hzr_16.F: 784 288
:geoo/construction/Laseremit_hzl_16.F: 736 288
:geoo/construction/Laseremit_hzr_16.F: 80 288
:geoo/construction/Laseremit_hzl_16.F: 32 288
:geoo/construction/sawblade.F: 32 336
:geoo/construction/sawblade.F: 48 352
:geoo/construction/sawblade.F: 16 320
:geoo/construction/sawblade.F: 784 320
:geoo/construction/sawblade.F: 768 336
:geoo/construction/sawblade.F: 752 352
:geoo/construction/sawblade.F: 736 352
:geoo/construction/sawblade.F: 64 352
:geoo/construction/sawblade.F: 80 352
:geoo/construction/sawblade.F: 720 352
:geoo/construction/sawblade.F: 704 352
:geoo/construction/sawblade.F: 96 352

:geoo/steel/32x64o.S: 512 336
:geoo/steel/32x16o.S: 544 384
:geoo/steel/32x16o.S: 576 384
:geoo/steel/32x16o.S: 640 384
:geoo/steel/32x64o.S: 704 272
:geoo/steel/32x64o.S: 704 144
:geoo/steel/32x64o.S: 704 16
:geoo/steel/32x64o.S: 704 -48
:geoo/steel/32x64o.S: 96 272
:geoo/steel/32x16o.S: 160 384
:geoo/steel/32x16o.S: 224 384
:geoo/steel/32x16o.S: 256 384
:geoo/steel/32x64o.S: 0 240
:geoo/steel/32x64o.S: 96 144
:geoo/steel/32x64o.S: 0 176
:geoo/steel/32x64o.S: 96 -48
:geoo/construction/concrete/032v: 320 368 rrr
:geoo/construction/concrete/032v: 448 368 r
:geoo/steel/32x64o.S: 288 336
:geoo/steel/32x64o.S: 128 144
:geoo/steel/32x64o.S: 160 144
:geoo/steel/32x64o.S: 160 80
:geoo/steel/32x64o.S: 192 80
:geoo/steel/32x64o.S: 608 80
:geoo/steel/32x64o.S: 640 144
:geoo/steel/32x64o.S: 640 80
:geoo/steel/32x64o.S: 672 144
:geoo/steel/32x64o.S: 448 144
:geoo/steel/32x64o.S: 544 192
:geoo/steel/32x64o.S: 544 112
:geoo/steel/32x64o.S: 576 192
:geoo/steel/32x64o.S: 576 112
:geoo/steel/32x64o.S: 224 192
:geoo/steel/32x64o.S: 224 112
:geoo/steel/32x64o.S: 256 192
:geoo/steel/32x64o.S: 256 112
:geoo/steel/32x64o.S: 320 208
:geoo/steel/32x64o.S: 352 208
:geoo/steel/32x64o.S: 352 144
:geoo/steel/32x64o.S: 480 208
:geoo/steel/32x64o.S: 480 144
:geoo/steel/32x64o.S: 448 208
:geoo/steel/32x64o.S: 320 144
:geoo/construction/pillar_bottom: 160 304
:geoo/construction/pillar_bottom: 192 304
:geoo/construction/pillar_bottom: 608 304
:geoo/construction/pillar_bottom: 640 304
:geoo/construction/pillar_bottom: 128 304
:geoo/construction/pillar_bottom: 672 304
:geoo/construction/concrete/032ha: 448 336
:geoo/construction/concrete/032hb: 320 336
:geoo/construction/concrete/032v: 160 320
:geoo/construction/concrete/032v: 640 320
:geoo/construction/concrete/016v: 512 192 rrr
:geoo/construction/concrete/016v: 512 144 rrr
:geoo/construction/concrete/016v: 288 192 rrr
:geoo/construction/concrete/016v: 288 144 rrr
:geoo/construction/concrete/016v: 432 368
:geoo/construction/concrete/016v: 384 368
:geoo/steel/32x64o.S: -16 112
:geoo/steel/32x64o.S: 0 48
:geoo/steel/32x64o.S: 800 240
:geoo/steel/32x64o.S: 800 176
:geoo/steel/32x64o.S: 816 112
:geoo/steel/32x64o.S: 800 48
:geoo/construction/concrete/032v: 672 80
:geoo/construction/concrete/032v: 704 80
:geoo/steel/32x64o.S: 96 16
:geoo/construction/concrete/032v: 128 80
:geoo/construction/concrete/032v: 96 80
:geoo/steel/64x64.S: 288 16
:geoo/steel/64x64.S: 480 16
:geoo/construction/concrete/032: 288 208
:geoo/construction/concrete/032: 288 240
:geoo/construction/concrete/032: 512 208
:geoo/construction/concrete/032: 512 240
:geoo/construction/concrete/016v: 256 256 rrr
:geoo/construction/concrete/016v: 544 256 rrr
:geoo/construction/concrete/016hd: 576 256
:geoo/construction/concrete/016hc: 224 256
:geoo/steel/32x16o.S: 160 304
:geoo/steel/32x16o.S: 640 304
:geoo/steel/32x32o.S: 352 48
:geoo/steel/32x32o.S: 448 48
:geoo/steel/32x16o.S: 496 0
:geoo/steel/32x16o.S: 304 0
