Steps to install Creative legacy Sound Card on Windows NT 4.0
~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~

WARNING : Please remove all previously installed legacy driver or PnP
      driver before you install.

1. Unzip the zip file into a floppy disk and insert the disk into the
   floppy drive (<Floppy_Drive>).

2. Click Start, Settings, Control Panel.

3. Open the "Multimedia" Icon in the Control Panel.

4. Select the "Devices" tab.

5. Click the "Add..." button.

6a. For Sound Blaster 16:
   --------------------------------------------------------
   a) Choose "Unlisted or Updated Driver"

   b) Enter the path name which contains OEMSETUP.INF:
     <Floppy_Drive>\

   c) Choose "Creative Tech. Sound Blaster 16"

   d) Click "OK".  If asked to install new or current driver, choose "New"

   e) Choose your current Base I/O address (220, 240, 260, 280).

   f) Choose you other settings (IRQ, DMA, MPU-401).

   g) Restart when prompted

6b. For Creative Advanced Wave Effects Synthesis for AWE 32:
   --------------------------------------------------------
   a) Choose "Unlisted or Updated Driver"

   b) Enter the path name which contains OEMSETUP.INF:
     <Floppy_Drive>\

   c) Choose "Creative Sound Blaster AWE32 MIDI Synth"

   d) Click "OK".  If asked to install new or current driver, choose "New"

   e) Restart when prompted

7. Your Sound Blaster card should be working properly at this point.  If you
   need to change the resources that your card is using, open the Multimedia
   Control Panel applet, select the "Devices" tab, select "Properties" for
   the Sound Blaster driver, and click on the "Settings" button.  This will
   bring up the same resource picking dialog that was invoked when installing
   the device.


Known issues
============
- Only a single installed Sound Blaster audio card is supported.
