Disk Benchmark NVME SSD V1.1.0 x64

SEQ1M Q8T1

Sequential 1 MiB - Queue Depth 8 - 1 Thread

This benchmark measures the sequential read and write performance of a
storage device using 1 MiB blocks.

It simulates large file transfers such as:

-   Copying movies
-   Backing up folders
-   Transferring ISO images
-   Editing large video files

------------------------------------------------------------------------

SEQ

Sequential

Data is read or written in continuous order without random access.

This represents the fastest access pattern for SSDs and HDDs.

------------------------------------------------------------------------

1M

1 MiB Block Size

Each read or write operation transfers 1 MiB (1,048,576 bytes).

Large blocks reduce overhead and better represent real-world large file
transfers.

------------------------------------------------------------------------

Q8

Queue Depth = 8

Up to 8 I/O requests are processed simultaneously.

Modern NVMe SSDs are designed to take advantage of multiple outstanding
requests, improving throughput.

------------------------------------------------------------------------

T1

1 Thread

The benchmark uses one software thread.

This measures the storage device itself rather than the CPU’s ability to
generate multiple workloads.

------------------------------------------------------------------------

What does this result represent?

SEQ1M Q8T1 primarily measures the maximum sustained throughput of the
storage device.

Typical operations include:

-   Copying large files
-   Video editing
-   Backup operations
-   ISO creation
-   Disk imaging

------------------------------------------------------------------------

Disk Benchmark NVME SSD V1.1.0 x64

Disk Benchmark NVME SSD V1.1.0 x64 measures the real performance of a selected folder
through the Windows file system, providing results that closely represent everyday file copy operations.
